NOT PROTECTIVELY MARKED – Revised Police Operational Advice and Security Industry Requirements for Response to Security Systems (FEB 2026)
APPENDIX S – ANNEXE A (February 2026)

BRITISH STANDARDS AND EUROPEAN NORMS

(Current issue unless stated – see notes)

BS 4737	Intruder Alarms in Buildings (mostly withdrawn see notes)

BS 7042	High Security (withdrawn see notes)

BS 8418	Remotely monitored detector activated CCTV Systems

Industry stakeholders and the NPCC SSG recognises the need to provide an interim update to BS 8418:2021 to reflect the practical and technological developments in portable Video Surveillance Systems (PVSS). As crime patterns, detection technologies and deployment environments have evolved, additional clarity is required to ensure these portable, and rapidly deployable systems continue to meet the performance expectations necessary to support police response and eligibility for a Unique Reference Number (URN).

The Industry Agreement IA 2401:2026 sets out concise supplementary recommendations covering system planning, risk assessment, system design, deployment, and monitoring of PVSS. 

It is to be read in conjunction with BS 8418:2021, and serves as best‑practice guidance for organisations deploying portable systems who seek to obtain or maintain a Police URN.

BS 5979	Alarm Receiving Centres (Category II) (withdrawn see notes)

BS 8591	Alarm Receiving Centres (not Intruder & Hold up Alarms) 

BS 6799	Wire free Alarms (withdrawn see notes)

BS 62676-4	Video surveillance systems for use in security applications – Part 4 Application Guidelines

BS 7858	Security screening of individuals employed in a security environment

PD 6662:2017	Scheme for the application of European Standards for intruder and Hold-Up Alarm systems  *

PD 6662:2010 	Scheme for the application of European Standards for intruder and Hold-Up Alarm systems (withdrawn see notes)  *

PD 6662:2004	Scheme for the application of European Standards for intruder and Hold-Up Alarm systems (withdrawn see notes)  *

IA 1501:2015	Industry agreement on PD 6662:2010

BS EN 50518		Monitoring and Alarm Receiving Centres	

BS EN 50131	Series Intruder & Hold up Alarms

BS EN 50136	Series Alarm Transmission systems

BS EN 50131-8 	Security Fog Devices (applies under PD 6662)

BS 8473	Management of False Alarms

BS 8243	Installation & configuration of Intruder & HUAs designed to generate confirmed alarm systems (applies under PD 6662)

BS 8484	Provision of Lone Worker Device Services

BS 8593           	Code of Practice for the deployment and use of body worn video

BS 9518	Code of Practice for processing of alarm signals by an Alarm Receiving Centre (when published)

Note: *     Where intruder and hold-up alarm equipment is removed and re-installed, it must:
a) only be re-installed for use by the original owner
b) be certificated to the same standard as the original installation 
c) be compliant with PD6662:2010 or PD6662:2017

British Standards Institution Drafts for Development (Latest Issue)

BS DD 242	High Security (withdrawn see notes)

BS DD 243	Applies under PD 6662:2004 (withdrawn see notes)

BS DD 244	Wire Free Alarms (withdrawn see notes)

BS DD 263	Alarms Systems Commissioning, Maintenance and remote support (applies Under PD 6662)

BS 9263:2016   	Alarms Systems Commissioning, Maintenance and remote support (applies Under PD 6662:2017)

DD CLC/TS 50131-7:2010	Alarm Systems – Intrusion Systems – Application Guidelines

DD CLC/TS 50131-7:2008	Applies under PD 6662:2010 (withdrawn see notes)

DD CLC/TS 50131-7:2003 	Applies under PD 6662:2004 (withdrawn see notes)

Notes:
Certain standards are in a period of “Dual running” with previous issues, and either current OR the previous issue may be acceptable for a specified, limited period.

Some older and withdrawn standards or parts of standards are still included in this list for the benefit of legacy systems that remain in service

Cyber Security Guidance

NPCC recognises the need to include cyber security as a holistic part of a security system and includes the following as best practice guidance to installers: 

1. CySPAG (Cyber Security Product Assurance Group) - Registered installer scheme (form 369 published by BSIA)
2. Cyber Essentials / Cyber Essential Plus
3. Payment Card Industry Data Security Standard (PCIDSS)

Dual-Path Signalling Failures

Due to the increase in dual-path signalling failures, the NPCC Security Systems Group recommend the following as best practice guidance to installers:
Guidance for the Prevention and Reduction of Dual-Path Alarm Transmission Types (Form 373 published by BSIA)

Notes:
At this time the above guidance is not mandatory for companies claiming compliance with NPCC requirements

BSIA manufacturer scheme for UK standards compliance for control equipment used on I&HAS – Form 375
Security equipment manufacturers UK scheme for 3rd party compliance – Intruder & Hold-up alarm systems – Form 375

The NPCC SSG recognises the value in 3rd party certification and compliance of products and services as a means of assuring the quality of equipment installed on premises requiring a police response and includes the scheme as best practice guidance to installers when choosing control equipment for use in I&HAS systems.

The BSIA’s Security equipment manufacturers UK scheme (Form 375) has been developed to take account of the need to provide compliance of control equipment at a UK level. The scheme provides for independent 3rd party compliance of UK (PD 6662 / BS 8243) Control equipment requirements using the technical services team within the BSIA. 

Manufacturers complying with the BSIA Security equipment manufacturers UK scheme for 3rd party certification will be issued a scheme certificate of compliance and be registered on the BSIA website.

Other schemes providing an equivalent independent compliance to UK standards may be used.
For further information, and a copy of the terms of the scheme, contact the BSIA on technical@bsia.co.uk 

Note: Currently the above scheme is not mandatory for companies claiming compliance with NPCC requirements


Legislation

The Clean Neighbourhood and Environment Act 2005 set out requirements for intruder alarms, keyholders and noise.
The Companies Act 1985, 1989 & 2006
Product Security and Telecommunications Infrastructure (PSTI) Act 2022

